**CISC Simulator - Team 1**

A CISC Simulator was developed using JAVA (JDK version 19).

Refer to Design\_Document.pdf for more information.

**How to Use GUI Simulator**

**Download the following files from the blackboard**

Team 1 CISC Simulator Part I CSCI6461Section10Fall2022October12022.zip will contain the below files:

CISCComputerSimulator.jar (inside dist folder)

Simulator.java (inside src folder)

README.docx

Design\_Document.pdf

**Preparation Instructions**

Prepare Environment for execution

NOTE: Please make sure your system is running on JDK version "^19".

Start Execution

Once the files are extracted from the zip folder, double-click on the CISCComputerSimulator.jar file.

Or

To run the project from the command line, go to the dist folder path and type the following: java -jar "CISCComputerSimulator.jar"

**Operation of the Simulator**

How to IPL

Clicking on the "IPL" button will take the IPL.txt file from the unzipped location.

Clicking on the "Custom IPL" button will open a Dialog box to select the IPL file that the user wants to select (It doesn't necessarily have to be named IPL.txt)

Starting location where the simulator executes code

Once the "IPL" button or "Custom IPL" is clicked, the first location mentioned in the first line of the txt file would be taken as the PC.

For eg. If the IPL.txt contains the below content:

0006 004F

000A 0009

0020 000A

The PC would have the value **0x0006**

How to Single Step

Clicking either "IPL" or "Custom IPL" will load the PC with the first memory address location, then Click on the "SS" button to Single Step.

or

If memory values have been manually stored, Load the PC value with the memory that needs to be Single Stepped, and then Click on the "SS" button.

How to Run the machine code

Clicking either "IPL" or "Custom IPL" will load the PC with the first memory location, then Click on the "Run" button to Run the machine till it Halt instruction is encountered.

or

If memory values have been manually stored, Load the PC value with the memory address from where the instruction should be run, and then Click on "Run" button.

Note: When Halt is encountered, HALT Led would glow up and the machine would stop.

How to read memory locations

Click on the Instruction toggle bits corresponding to the memory address and Click on LD corresponding to MAR.

Click on the "Load" button, and MBR will be loaded with the value/instruction stored in MAR.

How to store memory

Click on the Instruction toggle bits corresponding to the memory address and Click on LD corresponding to MAR.

Click on the Instruction toggle bits corresponding to the value/instruction and Click on LD corresponding to MBR.

Click on the "Store" button, MAR will be stored with the value/instruction stored in MBR.

Clicking on "Store+" instead of "Store" will do the same operation as Store, in addition to that it'll also increment the MAR.